




MATERIAL DECLARATION (MD)

<Date of declaration>
	Date
	
	

	                                              <Supplier (respondent) information>

	<MD identification number>
	Company name
	

	ID-No.
	
	
	Division name
	

	<Other information>
	Address
	

	
	Contact person
	

	Remark 1
	
	
	Telephone number
	

	Remark 2
	
	
	Fax number
	

	Remark 3
	
	
	Email address
	

	
	SDoC ID number
	

	<Product information>

	Product name
	Product number
	Delivered unit
	Product information

	
	
	Amount
	Unit
	

	
	
	
	
	

	<Materials information>

	
	Unit
	

	This materials information shows the amount of hazardous materials contained in
	1
	
	(Unit: kg, m, m2, m3, piece, etc.) of the product

	
	
	

	Table
	Material name
	Threshold value
	Present above threshold value?
	If yes, material mass
	If yes, information on where it is used

	
	
	
	Yes  /  No
	Mass
	Unit
	

	Table A
(materials listed in
appendix 1 of the
Convention) and AFS Convention
	Asbestos
	Asbestos
	0.1% *
	
	
	
	

	
	Polychlorinated biphenyls (PCBs)
	Polychlorinated biphenyls (PCBs)
	50 mg/kg
	
	
	
	

	
	Ozone Depleting 
Substance (ODS)
	Chlorofluorocarbons (CFCs)
	No threshold value
	
	
	
	

	
	
	Halons
	
	
	
	
	

	
	
	Other fully halogenated CFCs
	
	
	
	
	

	
	
	Carbon tetrachloride 
	
	
	
	
	

	
	
	1, 1, 1-Trichloroethane
	
	
	
	
	

	
	
	Hydrochlorofluorocarbons
	
	
	
	
	

	
	
	Hydrobromofluorocarbons
	
	
	
	
	

	
	
	Methyl bromide
	
	
	
	
	

	
	
	Bromochloromethane
	
	
	
	
	

	
	Anti-fouling systems  containing organotin
compounds as a biocide
	e.g. Tributyltin (TBT)
	2500 mg total tin/kg
	
	
	
	

	
	
	e.g. Triphenyl tins (TPTs)
	
	
	
	
	

	
	
	e.g. Tributyltin oxide (TBTO)
	
	
	
	
	

	
	Cybutryne
	Cybutryne
	200 mg/kg
	
	
	
	

	EU SRR **
	Perfluorooctane sulfonic acid (PFOS)
	10 mg/kg
	
	
	
	

	



	Table
	Material name
	Threshold value
	Present above threshold value?
	If yes, material mass
	If yes, information on where it is used

	
	
	
	Yes  /  No
	Mass
	Unit
	

	Table B
(materials listed in 
appendix 2 of the 
Convention)
	Cadmium and cadmium compounds
	100 mg/kg
	
	
	
	

	
	Hexavalent chromium and hexavalent chromium compounds
	1000 mg/kg
	
	
	
	

	
	Lead and lead compounds
	1000 mg/kg
	
	
	
	

	
	Mercury and mercury compounds
	1000 mg/kg
	
	
	
	

	
	Polybrominated biphenyl (PBBs)
	50 mg/kg
	
	
	
	

	
	Polybrominated diphenyl ethers (PBDEs)
	1000 mg/kg
	
	
	
	

	
	Polychloronaphthalenes (Cl >=3)
	50 mg/kg
	
	
	
	

	
	Radioactive substances
	No threshold value
	
	
	
	

	
	Certain shortchain chlorinated paraffins
	1%
	
	
	
	

	EU SRR **
	Brominated flame retardant (HBCDD)
	100 mg/kg
	
	
	
	

	
*  In accordance with regulation 4 of the IMO Hong Kong Convention, for all ships, new installation of materials which contain asbestos shall be prohibited. 
According to the UN recommendation "Globally Harmonized System of Classification and Labelling of Chemicals (GHS)" adopted by the United Nations Economic and Social Council's Sub-Committee of Experts on the Globally Harmonized System of Classification and Labelling of Chemicals (UNSCEGHS), the UN's Sub Committee of Experts, in 2002 (published in 2003), carcinogenic mixtures classified as Category 1A (including asbestos mixtures) under the GHS are required to be labelled as carcinogenic if the ratio is more than 0.1%. However, if 1% is applied, this threshold value should be recorded in the Inventory and, if available, the Material Declaration and can be applied not later than five years after the entry into force of the Convention. The threshold value of 0.1% need not be retroactively applied to those Inventories and declarations.
** Additional materials to be listed, in accordance with Annex I and Annex II of the European Union Ship Recycling Regulation (Regulation (EU) No 1257/2013 Yes
No



This MD is to be completed in accordance with IMO Resolution MEPC.379(80) and should be accompanied by a Supplier's Declaration of Conformity (SDoC)








 SUPPLIER'S DECLARATION OF CONFORMITY FOR MATERIAL DECLARATION MANAGEMENT

1. SDoC Identification Number		

2. Issuer’s Name

Issuer’s Address



3. Object(s) of the Declaration



4. The object(s) of the declaration described above is in conformity with the following documents:

Document No.		Title									Edition/Date of Issue

 MEPC.379(80)		Guidelines for the development of the Inventory of Hazardous Materials	2023/07/07
 EU SRR			Regulation (EU) No 1257/2013 						2013/11/20
 EMSA			Best Practice Guide on the IHM						2016/10/28
 AFS Convention		Control of Harmful AFS on ships, 2001 with amendments 2021		2001/10/05
 MEPC.405(83)		Amendments for the development of the Inventory of Hazardous Materials	2025/04/11

5. Additional Information	


6. Signed for and on behalf of


    Place and date of Issue

7.  
    (Name, Function)						(Signature)

This SDoC is to be completed in accordance with IMO Resolution MEPC.379(80) and should be accompanied by one or more Material Declarations (MD)
